************************************************************
************************************************************
*  Installation Readme for Intel(R) Rapid Storage 
*  Technology enterprise (Intel(R) RSTe).
*
*  Refer to the system requirements for the operating 
*  systems supported by Intel(R) Rapid Storage Technology
*  enterprise.
*
*  This document makes references to products developed by
*  Intel(R). There are some restrictions on how these products
*  may be used, and what information may be disclosed to
*  others. Please read the Disclaimer section at the bottom
*  of this document, and contact your Intel(R) field
*  representative if you would like more information.
*
************************************************************
************************************************************

************************************************************
*  Intel(R) is making no claims of usability, efficacy or 
*  warranty. The INTEL(R) SOFTWARE LICENSE AGREEMENT contained
*  herein completely defines the license and use of this 
*  software.
************************************************************

************************************************************
*  CONTENTS OF THIS DOCUMENT
************************************************************

1. Overview
2. System Requirements
3. Language Support
4. Installing the Software
5. Verifying Installation of the Software
6. Advanced Installation Instructions
7. Identifying the Software Version Number
8. Uninstalling the Software
9. Entering the Pre-boot User Interface
Disclaimer
Intel(R) Software License Agreement

************************************************************
* 1.  OVERVIEW
************************************************************

Intel(R) Rapid Storage Technology enterprise (Intel(R) RSTe) is
designed to provide functionality for the following Storage
Controllers:

    SCU Controllers:
    - Intel(R) C600 series chipset SAS RAID (SATA mode) 
      Controller
    - Intel C600 series chipset SAS RAID Controller

    SATA RAID Controllers:
    - Intel(R) C600+/C220+ series chipset SATA RAID Controller

    SATA AHCI Controllers:
    - Intel(R) C600+/C220+ series chipset SATA AHCI Controller
    
************************************************************
* 2.  SYSTEM REQUIREMENTS
************************************************************

A. The system must be running on one of the following
   operating systems:

  - Microsoft Windows* 7
  - Microsoft Windows* 7 x64-bit Edition
  - Microsoft Windows* Server 2008 R2**
  - Microsoft Windows* Server 2008**
  - Microsoft Windows* Server 2008 x64-bit Edition**
  - Microsoft Windows* Server 2003 R2 SP2 x64-bit Edition**
  - Microsoft Windows* 8
  - Microsoft Windows* 8 x64-bit Edition
  - Microsoft Windows* Server 2012**
  - Microsoft Windows* Server 2012 x64-bit Edition**

  *  Other names and brands may be claimed as the property
     of others.
  ** Applies to all editions (for example 'Datacenter',
     'Web', etc.). Intel(R) RSTe, however, is only validated
      against the 'Enterprise' edition.

B. The following operating systems are not supported:

   Any operating system not listed in section 2.A.

C. The system should contain, at the very least, the minimum
   system memory required by the operating system.

************************************************************
* 3.  LANGUAGE SUPPORT
************************************************************

Below is a list of the languages (and their abbreviations)
for which the Intel(R) Rapid Storage Technology enterprise
software has been localized. The language code is listed in
parentheses preceding each language.

(0401) ARA: Arabic (Saudi Arabia)
(0804) CHS: Chinese (Simplified)
(0404) CHT: Chinese (Traditional)
(0405) CSY: Czech
(0406) DAN: Danish
(0413) NLD: Dutch
(0409) ENU: English (United States)
(040B) FIN: Finnish
(040C) FRA: French (International)
(0407) DEU: German
(0408) ELL: Greek
(040D) HEB: Hebrew
(040E) HUN: Hungarian
(0410) ITA: Italian
(0411) JPN: Japanese
(0412) KOR: Korean
(0414) NOR: Norwegian
(0415) PLK: Polish
(0416) PTB: Portuguese (Brazil)
(0816) PTG: Portuguese (Standard)
(0419) RUS: Russian
(0C0A) ESP: Spanish
(041D) SVE: Swedish
(041E) THA: Thai
(041F) TRK: Turkish

************************************************************
* 4.  INSTALLING THE SOFTWARE
************************************************************

A. General installation notes:

  1. To install Intel(R) Rapid Storage Technology enterprise,
     double-click on the self-extracting and self-installing
     setup file and answer all prompts presented.

  2. By default, all installed files (readme.txt, help,
     etc.) are copied to one of the following paths:
    
<bootdrive>\Program Files\Intel\Intel(R) Rapid Storage Technology enterprise

<bootdrive>\Program Files (x86)\Intel\Intel(R) Rapid Storage Technology enterprise

B. Windows Automated Installer* installation from hard drive
   or CD-ROM:
 
Note: This method will install the drivers for both the SAS 
      RAID and SATA RAID controllers.

  1. Download the Intel(R) Rapid Storage Technology enterprise
     setup file and double-click to self-extract and to
     begin the setup process.

  2. When the 'Welcome' window appears, click 'Next' to
     continue.
 
  3. When the 'Uninstallation Warning' window appears,
     please read the information provided, then click 'Next'
     to continue.

  4. When 'Software License Agreement' window appears, if
     you agree to these terms, click 'Yes' to continue.
     Otherwise, click 'No' to cancel the installation.

  5. When the 'Readme File Information' window appears,
     please read the information provided, then click
     'Next' to continue.

  6. The 'Setup Progress' window appears and displays the
     actions being performed for the installation.

  7. When the Windows Automated Installer*
     'Setup Is Complete' window appears, the following
      options display: 

    a. Make sure any open documents are saved, select
       'Yes, I want to restart my computer now.', then click
       'Finish'.

    b. Or select 'No, I want to restart later', then click
       'Finish'.

C. Driver pass-through (non-RAID) installation during Windows* 
   Server 2003 Edition using the 'F6 Method'+:

Note: This procedure will install only the software
      necessary for Windows* to install onto a single 
      pass-through (non-RAID Volume) disk and be functional.
      To install the remaining software, it is necessary to
      use the installation procedure outlined in Section 4.B
      once Windows* has completed it's installation.

Note: If the CD/DVD device is connected to the AHCI Controller 
      and the AHCI Controller is in RAID Mode and the boot
      device is on the SCU Controller, both 2a and 2b
      below will need to be followed (i.e. two floppy disks
      are required).

  1. Obtain the necessary files by one of two methods: 

    a. Download the latest Intel(R) RSTe F6 drivers from
       www.intel.com and extract the contents from the
       .zip file.

    b. Extract the files from the installation package. 
       See Section 6.B for instructions on extracting the
       files.

  2. Create a floppy (or USB key) containing the following
     files in the root directory:

    a. The files required if loading a driver for the SATA
       RAID controller is desired:

      - iaStorA.inf
      - iaAHCI.inf
      - iaStorA.sys
      - iaahci.cat
      - iaStorF.sys
      - txtsetup.oem

    b. The files required if loading a driver for the SAS
       RAID controller is desired:

      - iaStorS.inf
      - iaStorS.sys
      - iaStorF.sys
      - iaStorS.cat
      - txtsetup.oem

  3. At the beginning of the operating system installation,
     press F6 to install a third party SCSI or RAID driver:

    - When prompted, select 'S' to Specify Additional Device.

  4. When prompted, insert the media (floppy or USB key)
     that was created in step 2 and press 'Enter'.

  5. At this point you should be presented with a selection
     for one of the controllers listed in the Overview of
     this document (Section 1) depending on your hardware
     version and configuration.

  6. Highlight the selection that is appropriate for the
     hardware in your system and press 'Enter'.

  7. Press 'Enter' again to continue. Leave the floppy disk
     in the system until the next reboot as the software
     will need to be copied from the floppy disk again when
     setup is copying files.

+ The 'F6 Method' refers to the key sequence used during
  Windows* XP or Windows* Server 2003 installation to signal
  that a third party device driver needs to be loaded.

D. Driver installation during Microsoft Windows* 7, Vista*,
   or Server 2008 Installation:

Note: This procedure will install only the software
      necessary for Windows* to install and be functional.
      To install the remaining software, it is necessary to
      use the installation procedure outlined in Section 4.B
      once Windows* has completed it's installation.

  1. Extract all driver files from the installation package.
     See Section 6.B for instructions on extracting the
     files.

  2. Add files listed in Section 4.C.2 to a USB key.

  3. Begin the Windows* installation, following the normal
     sequence of events.

  4. When the 'Where do you want to install Windows?' window
     displays, plug in your USB key and click 'Load Driver'
     at the bottom left hand side of the window.

  5. When the 'Load Driver' dialog window displays, click
     'Browse'.

  6. When the 'Open' dialog window displays, navigate to the
     location of the installation files, click 'OK'.

  7. At this point, you should be presented with a selection
     for one of the controllers listed in the Overview
     of this document (Section 1), being dependent on your
     hardware version and configuration.

  8. Select the controller that is appropriate for the
     hardware in your system and click 'Next'.

  9. Proceed with the selection of your installation disk
     and complete the Windows* installation.

************************************************************
* 5.  VERIFYING INSTALLATION OF THE SOFTWARE
************************************************************

A. If installed via the Windows* Automated Installer:

  1. From the Windows* desktop, at the bottom left corner
     select 'Start' -> 'All Programs' -> 'Intel'.

  2. Locate and select 
     'Intel(R) Rapid Storage Technology enterprise'.

  3. The Intel(R) Rapid Storage Technology enterprise
     application should launch.

  4. If the application does not launch, the
     Intel(R) Rapid Storage Technology enterprise driver was
     not installed properly and setup needs to be run again.

B. If installed during Windows* Server 2003 Edition Installation.
   NOTE: Review the release notes included in this release for 
         instructions on installing the Microsoft* Hot Fix.  This
         HOT Fix MUST be applied before continueing.

  1. Install the Microsoft* Hot Fix patch outlined in the 
     release notes included in this release.

  2. From the 'Start' menu, select the 'Control Panel'.    

  3. Double-click the 'System' icon (you might first need to
     select 'Switch to Classic View' to make the 'System'
     icon available).

  4. On the dialog window that opens, select the 'Hardware'
     tab, then click 'Device Manager'.

  5. On the dialog window that opens, expand the
     'SCSI and RAID Controllers' entry.

  6. Under 'SCSI and RAID Controllers' there should be at
     least one of the following entries (depending on which
     driver was installed):

    - 'Intel(R) C600 Series Chipset SAS RAID (SATA Mode)
      Controller'
    - 'Intel(R) C600 Series Chipset SAS RAID Controller'
    - 'Intel(R) C600 Series Chipset SATA RAID Controller'

C. If installed during Microsoft Windows* 7, Vista*,
   or Server 2008 Installation:

  1. From the 'Start' menu, select the 'Control Panel'.

  2. On the dialog window that opens, double-click the
     'Device Manager' icon (you may first need to select 
     either 'Small icons' or 'Large icons' from the 
     'View by:' entry at the top right corner of the window 
     for Microsoft Windows* 7 or Server 2008, or click 
     'Classic View' in the left pane for Windows* Vista, to 
     make the 'Device Manager' icon visible).

  3. On the dialog window that opens, expand the
     'Storage controllers' entry.

  4. Under 'Storage controllers' there should be at least
     one of the following entries (depending on which
     driver was installed):

    - 'Intel(R) C600 Series Chipset SAS RAID (SATA Mode)
      Controller'
    - 'Intel(R) C600 Series Chipset SAS RAID Controller'
    - 'Intel(R) C600 Series Chipset SATA RAID Controller'

************************************************************
* 6.  ADVANCED INSTALLATION INSTRUCTIONS
************************************************************

A. Available setup flags:

  -?
  Presents a dialog showing all the supported setup flags. 

  -a
  Extracts drivers and readme files.

  -b
  Reboots the system without prompting after the setup
  completes.

  -g <LCID>
  Specifies the language of the setup dialogs (See section 3
  for a table listing valid LCID values for supported
  languages).

  -nodrv
  Does not install Intel(R) RSTe drivers.

  -nogui
  Does not create a start menu shortcut for the UI console.

  -noservice
  Does not install the Event Monitor Service.

  -notray
  Does not install the tray icon.

  -overwrite
  Ignores the overwrite warning.

  -p <path>
  Changes default directory location for application files.

  -report <path>
  Changes the default log path.

  -s
  Silent install (does not display any setup dialogs).

  -ver
  Displays driver versions.

Note: Flags and their parameters are not case-sensitive.

B. Extracting the necessary driver files for use during
   Windows* installation:

   Run the installation application with the -a and -p
   flags.

   Example: setup.exe -a -p c:\RSTe_files

            All required driver files will be placed into
            c:\RSTe_files

************************************************************
* 7.  IDENTIFYING THE SOFTWARE VERSION NUMBER
************************************************************

A. Version of the software installed via the Windows*
   Automated Installer:

  1. From the Windows* desktop, at the bottom left corner
     select 'Start' -> 'All Programs' -> 'Intel'.

  2. Locate and select 
     'Intel(R) Rapid Storage Technology enterprise'.

  3. When the Intel(R) Rapid Storage Technology enterprise
     application launches, click 'Help'.

  4. On the dialog window that opens, click 'About'.

  5. The version of the driver is displayed at the bottom
     of the window.

B. Version of the drivers on Windows* XP x64-bit Edition
   or Windows* Server 2003 Edition:

  1. From the 'Start' menu, select 'Control Panel'.    

  2. Double-click the 'System' icon (you might first need to
     select 'Switch to Classic View' to make the 'System'
     icon available).

  3. On the dialog window that opens, select the 'Hardware'
     tab, then click 'Device Manager'.

  4. On the dialog window that opens, expand the
     'SCSI and RAID Controllers' entry.

  5. Under 'SCSI and RAID Controllers', there should be at
     least one of the following entries (depending on which
     drivers are installed):

    - 'Intel(R) C600 Series Chipset SAS RAID (SATA Mode)
      Controller'
    - 'Intel(R) C600 Series Chipset SAS RAID Controller'
    - 'Intel(R) C600 Series Chipset SATA RAID Controller'
    - 'Intel(R) C600 Series Chipset SATA AHCI Controller'

  6. Right click and select 'Properties' on one of the
     entries listed under 'SCSI and RAID Controllers'.

  7. On the dialog window that opens, click on the 'Driver'
     tab and look for the entry 'Driver Version'.

C. Version of the drivers on Microsoft Windows* 7, Vista*,
   or Server 2008.

  1. From the 'Start' menu, select the 'Control Panel'.

  2. On the dialog window that opens, double-click the
     'Device Manager' icon (you may first need to select 
     either 'Small icons' or 'Large icons' from the 
     'View by:' entry at the top right corner of the window 
     for Microsoft Windows* 7 or Server 2008, or click 
     'Classic View' in the left pane for Windows* Vista, to 
     make the 'Device Manager' icon visible).

  3. On the dialog window that opens, expand the
     'Storage controllers' entry.

  4. Under 'Storage controllers', there should be at least
     one of the following entries (depending on which
     driver are installed):

    - 'Intel(R) C600 Series Chipset SAS RAID (SATA Mode)
      Controller'
    - 'Intel(R) C600 Series Chipset SAS RAID Controller'
    - 'Intel(R) C600 Series Chipset SATA RAID Controller'
    - 'Intel(R) C600 Series Chipset SATA AHCI Controller'

  5. Right click and select 'Properties' on one of the
     entries listed under 'Storage controllers'.

  6. On the dialog window that opens, click on the 'Driver'
     tab and look for the entry 'Driver Version'.

************************************************************
* 8.  UNINSTALLING THE SOFTWARE
************************************************************

WARNING: The removal of the device driver components of the
         Intel(R) RSTe software package may leave the system
         inoperable and any data inaccessible. Before
         attempting to remove any software, make sure all
         data has been backed up. Please consult the
         appropriate Microsoft Windows* documentation for
         your operating system regarding procedures on
         removing device drivers.

A. Uninstallation of non-driver components:

  Non-driver components of Intel(R) RSTe software package
  include the Intel(R) Control Center, 'Start' menu links,
  help files, and Taskbar notifications. The removal of
  this software will not affect system operability. The
  ability to create, delete, or modify existing RAID volumes
  created with the Intel(R) RSTe software from within
  Microsoft Windows*, however, will not be available.

B. Microsoft Windows* XP x64-bit Edition or 
   Windows* Server 2003 Edition.

  1. On the 'Start menu', select 'Control Panel'.

  2. Click 'Add or Remove Programs'. 

  3. Locate and select
    'Intel(R) Rapid Storage Technology enterprise'.

  4. Click 'Remove'.

  5. The uninstall will start. Follow any instructions
     presented during this process.

C. Microsoft Windows* 7, Vista*, or Server 2008:

  1. On the 'Start menu', select 'Control Panel'.

  2. Click 'Uninstall a program'.

  3. Locate and select
     'Intel(R) Rapid Storage Technology enterprise'.

  4. Right-click the application name, and then click
     'Uninstall'.

  5. The uninstall will start. Follow any instructions
     presented during this process.

************************************************************
* 9.  ENTERING THE PRE-BOOT USER INTERFACE
************************************************************

WARNING: An interface is provided to create and delete RAID
         volumes before Windows* boots. It is possible to
         render a system inoperable by use of this interface
         and extreme caution is advised when in use.
  
Press 'CTRL-I' when the 'Intel(R) Rapid Storage Technology 
enterprise' banner screen appears.

************************************************************
* DISCLAIMER
************************************************************

INFORMATION IN THIS DOCUMENT IS PROVIDED IN CONNECTION WITH
INTEL PRODUCTS.  NO LICENSE, EXPRESS OR IMPLIED, BY ESTOPPEL
OR OTHERWISE, TO ANY INTELLECTUAL PROPERTY RIGHTS IS GRANTED
BY THIS DOCUMENT. EXCEPT AS PROVIDED IN INTEL'S TERMS AND
CONDITIONS OF SALE FOR SUCH PRODUCTS, INTEL ASSUMES NO
LIABILITY WHATSOEVER AND INTEL DISCLAIMS ANY EXPRESS OR
IMPLIED WARRANTY, RELATING TO SALE AND/OR USE OF INTEL
PRODUCTS INCLUDING LIABILITY OR WARRANTIES RELATING TO
FITNESS FOR A PARTICULAR PURPOSE, MERCHANTABILITY, OR
INFRINGEMENT OF ANY PATENT, COPYRIGHT OR OTHER INTELLECTUAL
PROPERTY RIGHT.

UNLESS OTHERWISE AGREED IN WRITING BY INTEL, THE INTEL
PRODUCTS ARE NOT DESIGNED NOR INTENDED FOR ANY APPLICATION
IN WHICH THE FAILURE OF THE INTEL PRODUCT COULD CREATE A
SITUATION WHERE PERSONAL INJURY OR DEATH MAY OCCUR.

Intel may make changes to specifications and product
descriptions at any time, without notice. Designers must not
rely on the absence or characteristics of any features or
instructions marked "reserved" or "undefined".  Intel
reserves these for future definition and shall have no
responsibility whatsoever for conflicts or incompatibilities
arising from future changes to them. The information here is
subject to change without notice. Do not finalize a design
with this information.

************************************************************
* INTEL(R) SOFTWARE LICENSE AGREEMENT
************************************************************

The products described in this document may contain design
defects or errors known as errata which may cause the
product to deviate from published specifications. Current
characterized errata are available on request.

Contact your local Intel sales office or your distributor
to obtain the latest specifications and before placing your
product order.

Copies of documents which have an order number and are
referenced in this document, or other Intel literature, may
be obtained by calling 1-800-548-4725, or go to: 
http://www.intel.com/#/en_us_01

Intel(R) is a trademark of Intel Corporation in the U.S.
and other countries.

* Other names and brands may be claimed as the property of
  others

Copyright (c) 2001-2012, Intel Corporation. All rights 
reserved.
